# Static Call Graph for image .\TCON_NEW.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Mon Aug 26 15:43:01 2019

### Maximum Stack Usage = 168 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ AVT_CONFIG_check ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ AVT_CONFIG_check ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 274 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> SPIx_Init
  - >> GPIO_USART_Init
  - >> SYS_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 106 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 44 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2S_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPIx_Init
  - >> GPIO_USART_Init
  - >> SYS_Init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> SPI_I2S_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> SPI_I2S_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> SPIx_Init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPIx_Init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 156 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> GPIO_USART_Init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> GPIO_USART_Init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> usart_sendbyte

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> usart_sendbyte

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  SystemInit (Thumb, 70 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> SYS_Init
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  Delay (Thumb, 18 bytes, Stack size 8 bytes, board.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay
  [Called By]
  - >> Delay100ms
  - >> Delay1ms

  Delay1ms (Thumb, 22 bytes, Stack size 4 bytes, board.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Delay1ms ⇒ Delay
  [Calls]
  - >> Delay
  [Called By]
  - >> tps_init
  - >> tps_sleep_to_standby
  - >> avt_lut_demo
  - >> avt_reset

  Delay100ms (Thumb, 20 bytes, Stack size 4 bytes, board.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Delay100ms ⇒ Delay
  [Calls]
  - >> Delay
  [Called By]
  - >> main
  - >> avt_init
  - >> AVT_CONFIG_check

  IO_Init (Thumb, 86 bytes, Stack size 0 bytes, board.o(.text))
  [Called By]

  - >> main
  - >> SYS_Init

  SYS_Init (Thumb, 192 bytes, Stack size 8 bytes, board.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = SYS_Init ⇒ SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> IO_Init
  - >> SystemInit
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  GPIO_USART_Init (Thumb, 124 bytes, Stack size 24 bytes, board.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = GPIO_USART_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  usart_sendbyte (Thumb, 28 bytes, Stack size 8 bytes, board.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = usart_sendbyte
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Called By]
  - >> Debug_str

  Debug_str (Thumb, 22 bytes, Stack size 8 bytes, board.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> usart_sendbyte
  [Called By]
  - >> tps_read_all_reg
  - >> i2c_ack
  - >> avt_init
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end
  - >> epd_draw_pic_start
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_start
  - >> avt_spi_flash_write_waveform_deal
  - >> avt_spi_flash_read_id
  - >> avt_spi_flash_read_buff
  - >> avt_spi_flash_write_buff
  - >> avt_spi_flash_deal_wait
  - >> avt_spi_flash_idle_wait
  - >> SpiFlash_StatusWait
  - >> Debug_dec
  - >> Debug_hex

  Debug_hex (Thumb, 156 bytes, Stack size 24 bytes, board.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Debug_hex ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> Debug_str
  [Called By]
  - >> tps_read_all_reg
  - >> avt_init
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_start
  - >> avt_spi_flash_write_waveform_deal
  - >> avt_spi_flash_read_id

  Debug_dec (Thumb, 130 bytes, Stack size 16 bytes, board.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Debug_dec ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> Debug_str
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_deal
  - >> avt_spi_flash_write_buff

  SPIx_Init (Thumb, 116 bytes, Stack size 32 bytes, board.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPIx_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Cmd
  - >> SPI_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  SpiFlash_ReadWriteByte (Thumb, 66 bytes, Stack size 0 bytes, driver.o(.text), UNUSED)
  [Called By]

  - >> epd_draw_pic_from_spiflash
  - >> SpiFlash_ReadData
  - >> SpiFlash_PageProgram
  - >> SpiFlash_EraseBlock32K
  - >> SpiFlash_StatusWait
  - >> SpiFlash_ReadID

  SpiFlash_ReadID (Thumb, 64 bytes, Stack size 4 bytes, driver.o(.text), UNUSED)
  [Calls]

  - >> SpiFlash_ReadWriteByte

  SpiFlash_StatusWait (Thumb, 54 bytes, Stack size 8 bytes, driver.o(.text), UNUSED)
  [Calls]

  - >> SpiFlash_ReadWriteByte
  - >> Debug_str
  [Called By]
  - >> SpiFlash_PageProgram
  - >> SpiFlash_EraseBlock32K

  SpiFlash_EraseBlock32K (Thumb, 100 bytes, Stack size 24 bytes, driver.o(.text), UNUSED)
  [Calls]

  - >> SpiFlash_StatusWait
  - >> SpiFlash_ReadWriteByte

  SpiFlash_PageProgram (Thumb, 122 bytes, Stack size 32 bytes, driver.o(.text), UNUSED)
  [Calls]

  - >> SpiFlash_StatusWait
  - >> SpiFlash_ReadWriteByte

  SpiFlash_ReadData (Thumb, 56 bytes, Stack size 20 bytes, driver.o(.text), UNUSED)
  [Calls]

  - >> SpiFlash_ReadWriteByte

  avt_delay (Thumb, 2 bytes, Stack size 0 bytes, epd.o(.text), UNUSED)

  avt_reset (Thumb, 28 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = avt_reset ⇒ Delay1ms ⇒ Delay
  [Calls]
  - >> Delay1ms
  [Called By]
  - >> avt_init
  - >> AVT_CONFIG_check

  avt_busy_wait (Thumb, 22 bytes, Stack size 0 bytes, epd.o(.text))
  [Called By]

  - >> avt_wait_dspe_lutfree
  - >> avt_wait_dspe_frend
  - >> avt_bst_wr_sdr
  - >> avt_bst_rd_sdr
  - >> avt_init_sys_run
  - >> avt_slp
  - >> avt_stby
  - >> avt_run_sys
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  - >> avt_i80_read_dat

  avt_i80_read_dat (Thumb, 84 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = avt_i80_read_dat
  [Calls]
  - >> avt_busy_wait
  [Called By]
  - >> avt_rd_reg

  avt_i80_write_dat (Thumb, 58 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = avt_i80_write_dat
  [Calls]
  - >> avt_busy_wait
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_buff
  - >> avt_upd_set_imgadr
  - >> avt_upd_part_area
  - >> avt_upd_part
  - >> avt_upd_full_area
  - >> avt_upd_full
  - >> avt_rd_wfm_info
  - >> avt_wait_dspe_mlutfree
  - >> avt_ld_img_setadr
  - >> avt_ld_img_area
  - >> avt_ld_img
  - >> avt_bst_wr_sdr
  - >> avt_bst_rd_sdr
  - >> avt_wr_sfm
  - >> avt_wr_reg_addr
  - >> avt_wr_reg
  - >> avt_rd_reg
  - >> avt_init_rotmode
  - >> avt_init_dspe_tmg
  - >> avt_init_dspe_cfg
  - >> avt_init_sdram
  - >> avt_init_pll_stby
  - >> avt_init_cmd_set

  avt_i80_write_cmd (Thumb, 54 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = avt_i80_write_cmd
  [Calls]
  - >> avt_busy_wait
  [Called By]
  - >> avt_upd_set_imgadr
  - >> avt_upd_gdrv_clr
  - >> avt_upd_part_area
  - >> avt_upd_part
  - >> avt_upd_full_area
  - >> avt_upd_full
  - >> avt_upd_init
  - >> avt_rd_wfm_info
  - >> avt_wait_dspe_mlutfree
  - >> avt_wait_dspe_lutfree
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_dspeadr
  - >> avt_ld_img_setadr
  - >> avt_ld_img_wait
  - >> avt_ld_img_end
  - >> avt_ld_img_area
  - >> avt_ld_img
  - >> avt_bst_end_sdr
  - >> avt_bst_wr_sdr
  - >> avt_bst_rd_sdr
  - >> avt_end_sfm
  - >> avt_wr_sfm
  - >> avt_rd_sfm
  - >> avt_wr_reg_addr
  - >> avt_wr_reg
  - >> avt_rd_reg
  - >> avt_init_rotmode
  - >> avt_init_dspe_tmg
  - >> avt_init_dspe_cfg
  - >> avt_init_sdram
  - >> avt_init_sys_stby
  - >> avt_init_sys_run
  - >> avt_slp
  - >> avt_stby
  - >> avt_run_sys
  - >> avt_init_pll_stby
  - >> avt_init_cmd_set

  avt_init_cmd_set (Thumb, 32 bytes, Stack size 8 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_init_pll_stby (Thumb, 34 bytes, Stack size 12 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_run_sys (Thumb, 18 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = avt_run_sys ⇒ avt_i80_write_cmd
  [Calls]
  - >> tps_source_gate_enable
  - >> avt_i80_write_cmd
  - >> avt_busy_wait
  [Called By]
  - >> main
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_start

  avt_stby (Thumb, 14 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_busy_wait

  avt_slp (Thumb, 22 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = avt_slp ⇒ avt_i80_write_cmd
  [Calls]
  - >> tps_vcom_disable
  - >> tps_source_gate_disable
  - >> avt_i80_write_cmd
  - >> avt_busy_wait
  [Called By]
  - >> main
  - >> avt_init
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  avt_init_sys_run (Thumb, 18 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = avt_init_sys_run ⇒ avt_i80_write_cmd
  [Calls]
  - >> tps_source_gate_enable
  - >> avt_i80_write_cmd
  - >> avt_busy_wait
  [Called By]
  - >> avt_init

  avt_init_sys_stby (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_init_sdram (Thumb, 40 bytes, Stack size 16 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_init_dspe_cfg (Thumb, 48 bytes, Stack size 20 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = avt_init_dspe_cfg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init

  avt_init_dspe_tmg (Thumb, 48 bytes, Stack size 20 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = avt_init_dspe_tmg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init

  avt_init_rotmode (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_rd_reg (Thumb, 26 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = avt_rd_reg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  - >> avt_i80_read_dat
  [Called By]
  - >> avt_init
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_start
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_idle_wait
  - >> avt_check_soft_ready

  avt_wr_reg (Thumb, 26 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = avt_wr_reg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_end
  - >> avt_spi_flash_write_waveform_start
  - >> avt_spi_flash_read_id
  - >> avt_spi_flash_read_buff
  - >> avt_spi_flash_write_page
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_earase
  - >> avt_spi_flash_write_disable
  - >> avt_spi_flash_write_enable
  - >> avt_spi_flash_read_status
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte

  avt_wr_reg_addr (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_wr_reg_addr ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_start

  avt_rd_sfm (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_wr_sfm (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_end_sfm (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_bst_rd_sdr (Thumb, 44 bytes, Stack size 16 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  - >> avt_busy_wait

  avt_bst_wr_sdr (Thumb, 44 bytes, Stack size 16 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  - >> avt_busy_wait

  avt_bst_end_sdr (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_ld_img (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_ld_img ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_start

  avt_ld_img_area (Thumb, 48 bytes, Stack size 20 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = avt_ld_img_area ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part

  avt_ld_img_end (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_ld_img_end ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  avt_ld_img_wait (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_ld_img_setadr (Thumb, 24 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_ld_img_setadr ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init

  avt_ld_img_dspeadr (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_wait_dspe_trg (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_wait_dspe_trg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  avt_wait_dspe_frend (Thumb, 14 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_wait_dspe_frend ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_busy_wait
  [Called By]
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  avt_wait_dspe_lutfree (Thumb, 14 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_wait_dspe_lutfree ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_busy_wait
  [Called By]
  - >> epd_draw_gray_part_lut

  avt_wait_dspe_mlutfree (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_rd_wfm_info (Thumb, 24 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_rd_wfm_info ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init

  avt_upd_init (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_upd_full (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_upd_full ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  avt_upd_full_area (Thumb, 58 bytes, Stack size 20 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = avt_upd_full_area ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part

  avt_upd_part (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_upd_part_area (Thumb, 48 bytes, Stack size 20 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat

  avt_upd_gdrv_clr (Thumb, 10 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_cmd

  avt_upd_set_imgadr (Thumb, 24 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = avt_upd_set_imgadr ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_i80_write_cmd
  - >> avt_i80_write_dat
  [Called By]
  - >> avt_init

  avt_check_soft_ready (Thumb, 18 bytes, Stack size 4 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_rd_reg

  avt_spi_flash_idle_wait (Thumb, 34 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_rd_reg
  - >> Debug_str
  [Called By]
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte

  avt_spi_flash_write_byte (Thumb, 26 bytes, Stack size 16 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_idle_wait
  - >> avt_wr_reg
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_read_id
  - >> avt_spi_flash_read_buff
  - >> avt_spi_flash_write_page
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_earase
  - >> avt_spi_flash_write_disable
  - >> avt_spi_flash_write_enable
  - >> avt_spi_flash_read_status

  avt_spi_flash_read_byte (Thumb, 30 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = avt_spi_flash_read_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_idle_wait
  - >> avt_wr_reg
  - >> avt_rd_reg
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_read_id
  - >> avt_spi_flash_read_buff
  - >> avt_spi_flash_read_status

  avt_spi_flash_read_status (Thumb, 38 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  [Called By]
  - >> avt_spi_flash_deal_wait

  avt_spi_flash_deal_wait (Thumb, 28 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_read_status
  - >> Debug_str
  [Called By]
  - >> avt_spi_flash_write_page
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_earase

  avt_spi_flash_write_enable (Thumb, 30 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = avt_spi_flash_write_enable ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  [Called By]
  - >> avt_spi_flash_write_page
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_earase

  avt_spi_flash_write_disable (Thumb, 30 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = avt_spi_flash_write_disable ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  [Called By]
  - >> avt_spi_flash_write_page
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_earase

  avt_spi_flash_earase (Thumb, 42 bytes, Stack size 8 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_spi_flash_write_disable
  - >> avt_spi_flash_write_enable
  - >> avt_spi_flash_deal_wait
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg

  avt_spi_flash_sector_earase (Thumb, 76 bytes, Stack size 24 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = avt_spi_flash_sector_earase ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_disable
  - >> avt_spi_flash_write_enable
  - >> avt_spi_flash_deal_wait
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_deal

  avt_spi_flash_write_page (Thumb, 96 bytes, Stack size 32 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_disable
  - >> avt_spi_flash_write_enable
  - >> avt_spi_flash_deal_wait
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  [Called By]
  - >> avt_spi_flash_write_buff

  avt_spi_flash_write_buff (Thumb, 66 bytes, Stack size 32 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_page
  - >> Debug_dec
  - >> Debug_str
  [Called By]
  - >> AVT_CONFIG_check
  - >> avt_spi_flash_write_waveform_deal

  avt_spi_flash_read_buff (Thumb, 92 bytes, Stack size 32 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  - >> Debug_str

  avt_spi_flash_read_id (Thumb, 84 bytes, Stack size 16 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = avt_spi_flash_read_id ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  - >> Debug_hex
  - >> Debug_str
  [Called By]
  - >> avt_spi_flash_write_waveform_start

  avt_spi_flash_write_waveform_deal (Thumb, 124 bytes, Stack size 24 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = avt_spi_flash_write_waveform_deal ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_buff
  - >> avt_spi_flash_sector_earase
  - >> Debug_dec
  - >> Debug_hex
  - >> Debug_str
  [Called By]
  - >> avt_waveform_update

  avt_spi_flash_write_waveform_start (Thumb, 68 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = avt_spi_flash_write_waveform_start ⇒ avt_spi_flash_read_id ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_read_id
  - >> avt_wr_reg
  - >> avt_rd_reg
  - >> Debug_hex
  - >> Debug_str
  [Called By]
  - >> avt_waveform_update

  avt_spi_flash_write_waveform_end (Thumb, 16 bytes, Stack size 4 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = avt_spi_flash_write_waveform_end ⇒ avt_wr_reg ⇒ avt_i80_write_cmd
  [Calls]
  - >> avt_wr_reg
  [Called By]
  - >> avt_waveform_update

  avt_waveform_update (Thumb, 16 bytes, Stack size 8 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = avt_waveform_update ⇒ avt_spi_flash_write_waveform_deal ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_waveform_end
  - >> avt_spi_flash_write_waveform_start
  - >> avt_spi_flash_write_waveform_deal
  [Called By]
  - >> main

  AVT_CONFIG_check (Thumb, 890 bytes, Stack size 32 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = AVT_CONFIG_check ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> avt_spi_flash_write_buff
  - >> avt_spi_flash_sector_earase
  - >> avt_spi_flash_read_byte
  - >> avt_spi_flash_write_byte
  - >> avt_wr_reg
  - >> avt_rd_reg
  - >> avt_reset
  - >> Debug_dec
  - >> Debug_hex
  - >> Debug_str
  - >> Delay100ms
  [Called By]
  - >> main

  epd_draw_pic_start (Thumb, 28 bytes, Stack size 8 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_ld_img
  - >> avt_wr_reg_addr
  - >> avt_run_sys
  - >> Debug_str

  epd_draw_pic_buff (Thumb, 52 bytes, Stack size 16 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> avt_i80_write_dat

  epd_draw_pic_end (Thumb, 44 bytes, Stack size 8 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> avt_upd_full
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_slp
  - >> Debug_str

  epd_draw_pic_from_spiflash (Thumb, 192 bytes, Stack size 40 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> avt_upd_full
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> SpiFlash_ReadWriteByte
  - >> Debug_str

  epd_draw_gray (Thumb, 130 bytes, Stack size 24 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = epd_draw_gray ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> tps_standby_to_sleep
  - >> tps_sleep_to_standby
  - >> avt_upd_full
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> Debug_str
  [Called By]
  - >> main
  - >> avt_init

  epd_draw_gray_level_horizontal (Thumb, 840 bytes, Stack size 32 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = epd_draw_gray_level_horizontal ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> tps_standby_to_sleep
  - >> tps_sleep_to_standby
  - >> avt_upd_full
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> Debug_str
  [Called By]
  - >> main

  epd_draw_gray_level_vertical (Thumb, 222 bytes, Stack size 32 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = epd_draw_gray_level_vertical ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> tps_standby_to_sleep
  - >> tps_sleep_to_standby
  - >> avt_upd_full
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> Debug_str
  [Called By]
  - >> main

  epd_draw_gray_part (Thumb, 168 bytes, Stack size 40 bytes, epd.o(.text), UNUSED)
  [Calls]

  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> tps_standby_to_sleep
  - >> tps_sleep_to_standby
  - >> avt_upd_full_area
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img_area
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> Debug_str

  epd_draw_pic_part_from_rom (Thumb, 286 bytes, Stack size 56 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = epd_draw_pic_part_from_rom ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_enable
  - >> tps_vcom_disable
  - >> tps_standby_to_sleep
  - >> tps_sleep_to_standby
  - >> avt_upd_full_area
  - >> avt_wait_dspe_frend
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img_area
  - >> avt_wr_reg_addr
  - >> avt_slp
  - >> avt_run_sys
  - >> avt_i80_write_dat
  - >> Debug_str
  [Called By]
  - >> main

  epd_draw_gray_part_lut (Thumb, 152 bytes, Stack size 40 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = epd_draw_gray_part_lut ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_enable
  - >> tps_sleep_to_standby
  - >> avt_upd_full_area
  - >> avt_wait_dspe_lutfree
  - >> avt_wait_dspe_trg
  - >> avt_ld_img_end
  - >> avt_ld_img_area
  - >> avt_wr_reg_addr
  - >> avt_i80_write_dat
  - >> Debug_str
  [Called By]
  - >> avt_lut_demo

  avt_lut_demo (Thumb, 1240 bytes, Stack size 24 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = avt_lut_demo ⇒ epd_draw_gray_part_lut ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> epd_draw_gray_part_lut
  - >> Delay1ms
  [Called By]
  - >> main

  avt_init (Thumb, 520 bytes, Stack size 16 bytes, epd.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = avt_init ⇒ epd_draw_gray ⇒ tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> epd_draw_gray
  - >> avt_upd_set_imgadr
  - >> avt_rd_wfm_info
  - >> avt_ld_img_setadr
  - >> avt_ld_img
  - >> avt_rd_reg
  - >> avt_init_dspe_tmg
  - >> avt_init_dspe_cfg
  - >> avt_init_sys_run
  - >> avt_slp
  - >> avt_reset
  - >> Debug_hex
  - >> Debug_str
  - >> Delay100ms
  [Called By]
  - >> main

  main (Thumb, 488 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = main ⇒ AVT_CONFIG_check ⇒ avt_spi_flash_write_buff ⇒ avt_spi_flash_write_page ⇒ avt_spi_flash_deal_wait ⇒ avt_spi_flash_read_status ⇒ avt_spi_flash_write_byte ⇒ avt_spi_flash_idle_wait ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_init
  - >> tps_sleep_to_standby
  - >> avt_init
  - >> avt_lut_demo
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> AVT_CONFIG_check
  - >> avt_waveform_update
  - >> avt_slp
  - >> avt_run_sys
  - >> SPIx_Init
  - >> GPIO_USART_Init
  - >> SYS_Init
  - >> IO_Init
  - >> Delay100ms
  [Called By]
  - >> __rt_entry_main

  i2c_delayus (Thumb, 22 bytes, Stack size 8 bytes, power.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = i2c_delayus
  [Called By]
  - >> i2c_read_byte
  - >> i2c_send_byte
  - >> i2c_sendack
  - >> i2c_ack
  - >> i2c_stop
  - >> i2c_start

  i2c_start (Thumb, 52 bytes, Stack size 4 bytes, power.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = i2c_start ⇒ i2c_delayus
  [Calls]
  - >> i2c_delayus
  [Called By]
  - >> I2C_Read_Frame
  - >> I2C_Write_Frame
  - >> I2C_Read
  - >> I2C_Write

  i2c_stop (Thumb, 40 bytes, Stack size 4 bytes, power.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = i2c_stop ⇒ i2c_delayus
  [Calls]
  - >> i2c_delayus
  [Called By]
  - >> I2C_Read_Frame
  - >> I2C_Write_Frame
  - >> I2C_Read
  - >> I2C_Write

  i2c_ack (Thumb, 90 bytes, Stack size 16 bytes, power.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> i2c_delayus
  - >> Debug_str
  [Called By]
  - >> I2C_Read_Frame
  - >> I2C_Write_Frame
  - >> I2C_Read
  - >> I2C_Write

  i2c_sendack (Thumb, 40 bytes, Stack size 4 bytes, power.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = i2c_sendack ⇒ i2c_delayus
  [Calls]
  - >> i2c_delayus
  [Called By]
  - >> I2C_Read_Frame

  i2c_send_byte (Thumb, 68 bytes, Stack size 8 bytes, power.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = i2c_send_byte ⇒ i2c_delayus
  [Calls]
  - >> i2c_delayus
  [Called By]
  - >> I2C_Read_Frame
  - >> I2C_Write_Frame
  - >> I2C_Read
  - >> I2C_Write

  i2c_read_byte (Thumb, 72 bytes, Stack size 4 bytes, power.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = i2c_read_byte ⇒ i2c_delayus
  [Calls]
  - >> i2c_delayus
  [Called By]
  - >> I2C_Read_Frame
  - >> I2C_Read

  I2C_Write (Thumb, 48 bytes, Stack size 16 bytes, power.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> i2c_send_byte
  - >> i2c_ack
  - >> i2c_stop
  - >> i2c_start
  [Called By]
  - >> tps_vposvneg_set
  - >> tps_vcom_set
  - >> tps_power_sequence_set

  I2C_Read (Thumb, 60 bytes, Stack size 16 bytes, power.o(.text), UNUSED)
  [Calls]

  - >> i2c_read_byte
  - >> i2c_send_byte
  - >> i2c_ack
  - >> i2c_stop
  - >> i2c_start
  [Called By]
  - >> ti_read_int_status

  I2C_Write_Frame (Thumb, 66 bytes, Stack size 24 bytes, power.o(.text), UNUSED)
  [Calls]

  - >> i2c_send_byte
  - >> i2c_ack
  - >> i2c_stop
  - >> i2c_start

  I2C_Read_Frame (Thumb, 90 bytes, Stack size 24 bytes, power.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_Read_Frame ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> i2c_read_byte
  - >> i2c_send_byte
  - >> i2c_sendack
  - >> i2c_ack
  - >> i2c_stop
  - >> i2c_start
  [Called By]
  - >> tps_read_all_reg

  tps_power_sequence_set (Thumb, 52 bytes, Stack size 8 bytes, power.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = tps_power_sequence_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> I2C_Write
  [Called By]
  - >> tps_init
  - >> tps_sleep_to_standby

  tps_vcom_set (Thumb, 44 bytes, Stack size 16 bytes, power.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> I2C_Write
  [Called By]
  - >> tps_init
  - >> tps_sleep_to_standby

  tps_vposvneg_set (Thumb, 14 bytes, Stack size 8 bytes, power.o(.text), UNUSED)
  [Calls]

  - >> I2C_Write

  ti_read_int_status (Thumb, 16 bytes, Stack size 8 bytes, power.o(.text), UNUSED)
  [Calls]

  - >> I2C_Read

  tps_read_all_reg (Thumb, 66 bytes, Stack size 24 bytes, power.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = tps_read_all_reg ⇒ I2C_Read_Frame ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> I2C_Read_Frame
  - >> Debug_hex
  - >> Debug_str
  [Called By]
  - >> tps_init

  tps_sleep_to_standby (Thumb, 30 bytes, Stack size 8 bytes, power.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = tps_sleep_to_standby ⇒ tps_vcom_set ⇒ I2C_Write ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_vcom_set
  - >> tps_power_sequence_set
  - >> Delay1ms
  [Called By]
  - >> main
  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray

  tps_standby_to_sleep (Thumb, 24 bytes, Stack size 0 bytes, power.o(.text))
  [Called By]

  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray

  tps_source_gate_enable (Thumb, 10 bytes, Stack size 0 bytes, power.o(.text))
  [Called By]

  - >> avt_init_sys_run
  - >> avt_run_sys

  tps_source_gate_disable (Thumb, 12 bytes, Stack size 0 bytes, power.o(.text))
  [Called By]

  - >> avt_slp

  tps_vcom_enable (Thumb, 10 bytes, Stack size 0 bytes, power.o(.text))
  [Called By]

  - >> epd_draw_gray_part_lut
  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end

  tps_vcom_disable (Thumb, 12 bytes, Stack size 0 bytes, power.o(.text))
  [Called By]

  - >> epd_draw_pic_part_from_rom
  - >> epd_draw_gray_part
  - >> epd_draw_gray_level_vertical
  - >> epd_draw_gray_level_horizontal
  - >> epd_draw_gray
  - >> epd_draw_pic_from_spiflash
  - >> epd_draw_pic_end
  - >> avt_slp

  tps_init (Thumb, 70 bytes, Stack size 8 bytes, power.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = tps_init ⇒ tps_read_all_reg ⇒ I2C_Read_Frame ⇒ i2c_ack ⇒ Debug_str ⇒ usart_sendbyte
  [Calls]
  - >> tps_read_all_reg
  - >> tps_vcom_set
  - >> tps_power_sequence_set
  - >> Delay1ms
  [Called By]
  - >> main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 218 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols